wolfSSL for Renesas RA Evaluation Kit (EK-RA6M3G)
=================================================

## Description

This directory contains e2studio projects targeted at the Renesas RA 32-bit MCUs.\
The example projects include a wolfSSL TLS 1.2 client and server.\
They also include benchmark and cryptography tests for the wolfCrypt library.

The wolfssl project contains both the wolfSSL and wolfCrypt libraries.\
It is built as a `Renesas RA C Library Project` and contains the Renesas RA\
configuration.

The other projects (benchmark, client, server and test) are built as a\
`Renesas RA C Project Using RA Library`, where the RA library is the wolfssl project.\
The wolfssl Project Summary is listed below and is relevant for every project.

#### Project Summary

`Board:   EK-RA6M3G`\
`Device:  R7FA6M3AH3CFC`\
`Toolchain:   GCC ARM Embedded`\
`FSP Version:   0.8.0`

##### Selected software components

`Board Support Package Common Files   v0.8.0`\
`Arm CMSIS Version 5 - Core (M)   v5.5.1`\
`Amazon FreeRTOS   v0.8.0`\
`RA6M3G-EK Board Support Files   v0.8.0`\
`Board support package for R7FA6M3AH3CFC   v0.8.0`\
`Board support package for RA6M3   v0.8.0`\
`Board support package for RA6M3   v0.8.0`\
`Amazon FreeRTOS - Memory Management - Heap 4   v0.8.0`\
`r_ether to FreeRTOS+TCP Wrapper   v0.8.0`\
`Ethernet       v0.8.0`\
`Ethernet PHY   v0.8.0`\
`FreeRTOS+TCP   v0.8.0`\
`Amazon FreeRTOS - Buffer Allocation 2   v0.8.0`


## Setup Steps

The project directories are missing files necessary to build the project.\
These files can be generated when creating a new Renesas RA Project.\
The following steps explain how to generate the missing files and where to place them.

1.) Create a 'dummy' Renesas RA C Library Project.
   + Click File->New->`RA C/C++ Project`
   + Click `Renesas RA C Library Project`. Click Next
   + Enter `dummy_library` as the project name. Click Next.
   + Under `Board: Custom User Board`, select `EK-RA6M3G`.
   + Under `RTOS: No RTOS`, select `Amazon FreeRTOS`.
   + Click Next. Select `Amazon FreeRTOS - Minimal - Static Allocation`
   + Click Finish.

2.) Create a 'dummy' Renesas RA C Project Using RA Library.
   + Click File->New->`RA C/C++ Project`
   + Click `Renesas RA C Project Using RA Library`. Click Next
   + Enter `dummy_app` as the project name. Click Next.
   + Under `RA library project`, select `dummy_library`.
   + Click Finish.

3.) Import all the wolfSSL Projects into e2studio workspace.
   + Click File->`Open Projects from File System`
   + Click `Directory...` to the right of Import source
   + Select the RA6M3G folder location that contains the projects\
      example path: wolfssl/IDE/Renesas/e2studio/RA6M3G
   + Deselect the Non-Eclipse project, RA6M3G, by clicking the checkbox\
      Only the folders with 'Eclipse project' under 'Import as' need to be selected.
  + Click Finish.

4.) Copy files from `dummy_library` into `wolfSSL_RA6M3G`
   + Expand the dummy_library and wolfSSL_RA6M3G projects\
     (Click the drop-down arrow to the left of the project name.)
   + Select and Copy the following folders/files inside dummy_library\
`       ra/`\
`       ra_gen/`\
`       ra_cfg/`\
`       script/`\
`       R7FA6M3AH3CFC.pincfg`\
`       RA6M3G-EK.pingcfg`
   + Paste the copied folders/files into wolfSSL_RA6M3G
   + The `dummy_library` project can now be deleted.
   + Generate Project Content.
     + Click `Open RA Configuration` in the top bar (Grey Settings Cog)
     + Click `Generate Project Content` at top right (Green Icon)
   + Build wolfSSL_RA6M3G.

5.) Copy files from `dummy_app` into `./IDE/Renesas/e2studio/RA6M3G/common/ra6m3g/`\
    **NOTE:** This may need to be done outside of the e2studio environment (e.g. File Explorer).
   + Select and Copy the followng folder inside dummy_app\
`         src/`\
`         script/`
   + Paste the copied folders into `./IDE/Renesas/e2studio/RA6M3G/common/ra6m3g/`\
`     (The test, benchmark, client and server projects link to this folder.)`
   + The `dummy_app` project can now be deleted.

6.) Setup Network Environment

        The client and server projects have defines inside their wolfssl_thread_entry.h.
        These defines (ucIPAddress ... ucDNSServerAddress) may need to be changed
        based on your internal network environment.  The g_ether0_mac_address is the default
        mac address found inside the RA configuration inside the wolfssl project.
        The client wolfssl_thread_entry.h has defines (SERVER_IP and DEFAULT_PORT) that
        will need to be changed based on the server you're trying to connect to over
        the ethernet connection.

## Build and Run

### Build Each Project
Right-Click each Project and select Build.

### Run wolfCrypt Test and Benchmark
1.) Right-Click the Project name.\
2.) Select `Debug As` -> `Renesas GDB Hardware Debugging`\
3.) Select J-Link ARM. Click OK.\
4.) Select R7Fa6M3AH. Click OK.

### Run the wolfSSL TLS Server Example.
1.) Right-Click the Project name.\
2.) Select `Debug As` -> `Renesas GDB Hardware Debugging`\
3.) Select J-Link ARM. Click OK.\
4.) Select R7Fa6M3AH. Click OK.\
5.) Run the following wolfSSL example client command inside the base of the wolfssl directory.

```
./examples/client/client -h "ucIPAddress" -p 11111 -A ./certs/1024/ca-cert.pem
```
**NOTE:** "ucIPAddress" is "192.168.1.241" by default. (See wolfssl_thread_entry.h)

### Run the wolfSSL TLS Client Example.
 1.) Run the following wolfSSL example server command inside the base of the wolfssl directory.

```
./examples/server/server -b -d -p 11111 -c ./certs/1024/server-cert.pem -k ./certs/1024/server-key.pem
```
**NOTE:** The port 11111 is the DEFAULT_PORT inside wolfssl_thread_entry.h.\
If DEFAULT_PORT was changed then the above command will need to match it.

 2.) Right-Click the Project name.\
 3.) Select `Debug As` -> `Renesas GDB Hardware Debugging`\
 4.) Select J-Link ARM. Click OK.\
 5.) Select R7Fa6M3AH. Click OK.


## Troubleshooting

* The commands for the example client/server assumes it is being run from the
  base directory of wolfssl.

* Enter "#define DEBUG_WOLFSSL" inside user_settings.h or wolfssl_thread_entry.c\
   to enable wolfssl debug messages to the Renesas Virtual Debug Console.
   
* Some linking errors can be caused by the e2studio project files needing to be rebuilt and freshened.
Right-Click a project, select Index, click Rebuild and then click Freshen Files. Repeat for each project.

[Support Forum](https://www.wolfssl.com/forums/)

Support Email: support@wolfssl.com


## Resources

[wolfSSL Website](https://www.wolfssl.com/)

[wolfSSL Wiki](https://github.com/wolfSSL/wolfssl/wiki)

[wolfSSL Manual](https://wolfssl.com/wolfSSL/Docs-wolfssl-manual-toc.html)

[wolfSSL API Reference](https://wolfssl.com/wolfSSL/Docs-wolfssl-manual-17-wolfssl-api-reference.html)

[wolfCrypt API Reference](https://wolfssl.com/wolfSSL/Docs-wolfssl-manual-18-wolfcrypt-api-reference.html)

[TLS 1.3](https://www.wolfssl.com/docs/tls13/)
